<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="76.2" y2="0" width="0" layer="20"/>
<wire x1="76.2" y1="0" x2="76.2" y2="44.45" width="0" layer="20"/>
<wire x1="76.2" y1="44.45" x2="0" y2="44.45" width="0" layer="20"/>
<wire x1="0" y1="44.45" x2="0" y2="0" width="0" layer="20"/>
<text>BPD v4.0</text>
<text>E. Mikhailov</text>
<text>May 2013</text>
<hole x="71.12" y="5.08" drill="4.2418"/>
<hole x="71.12" y="39.37" drill="4.2418"/>
<hole x="5.08" y="39.37" drill="4.2418"/>
</plain>
<libraries>
<library name="evmik_rcl">
<packages>
<package name="1206">
</package>
<package name="0805">
</package>
<package name="POL1206">
</package>
</packages>
</library>
<library name="evmik_connectors_3pin">
<packages>
<package name="3_PIN_THRUGH_HOLE_LABELED">
</package>
</packages>
</library>
<library name="evmik_opamp">
<packages>
<package name="SOIC8">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
</packages>
</library>
<library name="evmik_trimmers">
<packages>
<package name="3386F">
</package>
</packages>
</library>
<library name="evmik_photodiodes">
<packages>
<package name="TO5">
</package>
</packages>
</library>
<library name="evmik_bnc_sma_connectors">
<packages>
<package name="CONN-BNC-AMP-TYPE3HORIZ">
<description>&lt;b&gt;BNC PCB &lt;u&gt;Horizontal&lt;/u&gt; mount connector&lt;/b&gt;, Amp, horizontal, 0.1" grid, types such as 227677-1.&lt;br&gt;
Don't forget the nut 1-329631-2 and maybe the shoulder washer 330620.&lt;br&gt;
Now with new &amp; improved mtg holes compared to ...TYPE2...!&lt;br&gt;
The section of the BNC hanging over the edge of the PCB is in layer 49 (Reference).&lt;br&gt;
http://catalog.tycoelectronics.com/TE/bin/TE.Connect?C=1&amp;PN=227677-1&amp;M=STARTSWITH&amp;LG=1&amp;I=13&amp;button.x=0&amp;button.y=0</description>
</package>
<package name="SMA-STRAIGHT">
</package>
</packages>
</library>
<library name="evmik_testpads">
<description>Testpads</description>
<packages>
<package name="13">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="evmik_opamp" package="SOIC8" value="ADA4817"/>
<element name="D1" library="evmik_photodiodes" package="TO5" value=""/>
<element name="D2" library="evmik_photodiodes" package="TO5" value=""/>
<element name="R1" library="evmik_rcl" package="1206" value="1 kOhm"/>
<element name="C3" library="evmik_rcl" package="POL1206" value="6.8uF"/>
<element name="R2" library="evmik_rcl" package="1206" value="1 kOhm"/>
<element name="+5V" library="evmik_testpads" package="13" value="TP-13"/>
<element name="-5V" library="evmik_testpads" package="13" value="TP-13"/>
<element name="IC2" library="evmik_opamp" package="SOIC8" value="OPA847"/>
<element name="R4" library="evmik_rcl" package="1206" value="49.9 Ohm"/>
<element name="R5" library="evmik_rcl" package="1206" value="750 Ohm"/>
<element name="R8" library="evmik_rcl" package="1206" value="0 Ohm"/>
<element name="R9" library="evmik_rcl" package="1206" value="0 Ohm"/>
<element name="R11" library="evmik_rcl" package="1206" value="15 kOhm"/>
<element name="C9" library="evmik_rcl" package="POL1206" value="6.8uF"/>
<element name="OFFSET" library="evmik_trimmers" package="3386F" value="10 kOhm"/>
<element name="AC1" library="evmik_bnc_sma_connectors" package="SMA-STRAIGHT" value=""/>
<element name="C1" library="evmik_rcl" package="0805" value="See notes"/>
<element name="C2" library="evmik_rcl" package="0805" value="120n"/>
<element name="C5" library="evmik_rcl" package="0805" value="120n"/>
<element name="C6" library="evmik_rcl" package="0805" value="120n"/>
<element name="C7" library="evmik_rcl" package="0805" value="120n"/>
<element name="C8" library="evmik_rcl" package="0805" value="120n"/>
<element name="C10" library="evmik_rcl" package="0805" value="See notes"/>
<element name="C4" library="evmik_rcl" package="0805" value="120n"/>
<element name="PWR" library="evmik_connectors_3pin" package="3_PIN_THRUGH_HOLE_LABELED" value=""/>
<element name="R7" library="evmik_rcl" package="1206" value="0 Ohm"/>
<element name="R10" library="evmik_rcl" package="1206" value="49.9 Ohm"/>
<element name="R12" library="evmik_rcl" package="1206" value="See notes"/>
<element name="C11" library="evmik_rcl" package="0805" value="2.2 uF"/>
<element name="R13" library="evmik_rcl" package="1206" value="49.9 Ohm"/>
<element name="AC2" library="evmik_bnc_sma_connectors" package="CONN-BNC-AMP-TYPE3HORIZ" value=""/>
<element name="DC1" library="evmik_bnc_sma_connectors" package="CONN-BNC-AMP-TYPE3HORIZ" value=""/>
<element name="R3" library="evmik_rcl" package="1206" value="10 Ohm"/>
<element name="R6" library="evmik_rcl" package="1206" value="10 Ohm"/>
<element name="R14" library="evmik_rcl" package="1206" value="10 Ohm"/>
<element name="R15" library="evmik_rcl" package="1206" value="10 Ohm"/>
<element name="GND" library="evmik_testpads" package="13" value="TP-13"/>
<element name="DC" library="evmik_testpads" package="13" value="TP-13"/>
<element name="AC" library="evmik_testpads" package="13" value="TP-13"/>
<element name="R16" library="evmik_rcl" package="1206" value="See notes"/>
<element name="AC3" library="evmik_bnc_sma_connectors" package="SMA-STRAIGHT" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="AC1" pad="G@1"/>
<contactref element="AC1" pad="G@2"/>
<contactref element="AC1" pad="G@3"/>
<contactref element="AC1" pad="G@4"/>
<contactref element="R2" pad="1"/>
<contactref element="C3" pad="-"/>
<contactref element="C9" pad="+"/>
<contactref element="PWR" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="D1" pad="P$3"/>
<contactref element="D2" pad="P$3"/>
<contactref element="AC2" pad="SHIELD2"/>
<contactref element="AC2" pad="SHIELD1"/>
<contactref element="DC1" pad="SHIELD2"/>
<contactref element="DC1" pad="SHIELD1"/>
<contactref element="GND" pad="TP"/>
<contactref element="AC3" pad="G@1"/>
<contactref element="AC3" pad="G@2"/>
<contactref element="AC3" pad="G@3"/>
<contactref element="AC3" pad="G@4"/>
</signal>
<signal name="-5V">
<contactref element="D2" pad="P$1"/>
<contactref element="-5V" pad="TP"/>
<contactref element="R8" pad="1"/>
<contactref element="C9" pad="-"/>
<contactref element="PWR" pad="3"/>
<contactref element="R6" pad="1"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="D1" pad="P$2"/>
<contactref element="+5V" pad="TP"/>
<contactref element="R9" pad="1"/>
<contactref element="C3" pad="+"/>
<contactref element="PWR" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="3"/>
<contactref element="R2" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="IIN">
<contactref element="IC1" pad="2"/>
<contactref element="D1" pad="P$1"/>
<contactref element="D2" pad="P$2"/>
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="VOUT">
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="6"/>
<contactref element="C1" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="DC1" pad="CONDUCTOR"/>
<contactref element="DC" pad="TP"/>
<contactref element="AC3" pad="1"/>
</signal>
<signal name="IIN1">
<contactref element="IC2" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="VOUT1">
<contactref element="IC2" pad="6"/>
<contactref element="C10" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="AC" pad="TP"/>
</signal>
<signal name="N$1">
<contactref element="R8" pad="2"/>
<contactref element="OFFSET" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="R11" pad="1"/>
<contactref element="OFFSET" pad="2"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R9" pad="2"/>
<contactref element="OFFSET" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="8"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="AC1" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="AC2" pad="CONDUCTOR"/>
</signal>
<signal name="N$10">
<contactref element="IC2" pad="3"/>
<contactref element="R13" pad="2"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="7"/>
<contactref element="R7" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="4"/>
<contactref element="C5" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="IC2" pad="7"/>
<contactref element="C8" pad="2"/>
<contactref element="R14" pad="1"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="IC2" pad="4"/>
<contactref element="C7" pad="2"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="IC2" pad="8"/>
<contactref element="R16" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
