<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="ev_mikhlaserlock">
<packages>
<package name="AD630">
</package>
</packages>
</library>
<library name="evmik_opamp">
<packages>
<package name="DIP8">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="evmik_rcl">
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="evmik_connectors_3pin">
<packages>
<package name="3_PIN_THRUGH_HOLE_LABELED">
</package>
</packages>
</library>
<library name="evmik_testpads">
<packages>
<package name="13">
</package>
</packages>
</library>
<library name="QuantumOptics">
<description>&lt;b&gt;U of T Physics, Quantum Optics Labs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by Alan Stummer, Nov '03&lt;/author&gt;&lt;p&gt;
Various devices, symbols and packages used here.</description>
<packages>
<package name="CONN-BNC-AMP-TYPE3HORIZ">
<description>&lt;b&gt;BNC PCB &lt;u&gt;Horizontal&lt;/u&gt; mount connector&lt;/b&gt;, Amp, horizontal, 0.1" grid, types such as 227677-1.&lt;br&gt;
Don't forget the nut 1-329631-2 and maybe the shoulder washer 330620.&lt;br&gt;
Now with new &amp; improved mtg holes compared to ...TYPE2...!&lt;br&gt;
The section of the BNC hanging over the edge of the PCB is in layer 49 (Reference).&lt;br&gt;
http://catalog.tycoelectronics.com/TE/bin/TE.Connect?C=1&amp;PN=227677-1&amp;M=STARTSWITH&amp;LG=1&amp;I=13&amp;button.x=0&amp;button.y=0</description>
</package>
</packages>
</library>
<library name="evmik_switches">
<packages>
<package name="SWITCH1AS">
</package>
</packages>
</library>
<library name="evmik_trimmers">
<packages>
<package name="3362S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="ev_mikhlaserlock" package="AD630" value="AD630"/>
<element name="INGN" library="evmik_opamp" package="DIP8" value=""/>
<element name="ALPS" library="evmik_opamp" package="DIP8" value=""/>
<element name="R5" library="evmik_rcl" package="1206" value="10k"/>
<element name="R7" library="evmik_rcl" package="1206" value="1k"/>
<element name="15_EXT2" library="evmik_connectors_3pin" package="3_PIN_THRUGH_HOLE_LABELED" value="15V_3PIN"/>
<element name="15V_EXT1" library="evmik_connectors_3pin" package="3_PIN_THRUGH_HOLE_LABELED" value="15V_3PIN"/>
<element name="C1" library="evmik_rcl" package="1206" value="1u"/>
<element name="OUT" library="evmik_opamp" package="DIP8" value=""/>
<element name="R1" library="evmik_rcl" package="1206" value="100k"/>
<element name="C2" library="evmik_rcl" package="1206" value="70uF"/>
<element name="LIOUT" library="evmik_testpads" package="13" value="TP-13"/>
<element name="PREAMP" library="evmik_testpads" package="13" value="TP-13"/>
<element name="PHASE" library="evmik_testpads" package="13" value="TP-13"/>
<element name="GND" library="evmik_testpads" package="13" value="TP-13"/>
<element name="R2" library="evmik_rcl" package="1206" value="1k"/>
<element name="INVT" library="evmik_opamp" package="DIP8" value=""/>
<element name="R3" library="evmik_rcl" package="1206" value="1k"/>
<element name="R4" library="evmik_rcl" package="1206" value="1k"/>
<element name="R6" library="evmik_rcl" package="1206" value="1k"/>
<element name="REFERENCE" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value=""/>
<element name="INPUT" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value=""/>
<element name="OUTPUT" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value=""/>
<element name="VIN" library="evmik_testpads" package="13" value="TP-13"/>
<element name="VREF" library="evmik_testpads" package="13" value="TP-13"/>
<element name="VOUT" library="evmik_testpads" package="13" value="TP-13"/>
<element name="INBUF" library="evmik_opamp" package="DIP8" value=""/>
<element name="C4" library="evmik_rcl" package="1206" value="22u"/>
<element name="R9" library="evmik_rcl" package="1206" value="1k"/>
<element name="R10" library="evmik_rcl" package="1206" value="100k"/>
<element name="R11" library="evmik_rcl" package="1206" value="100k"/>
<element name="C5" library="evmik_rcl" package="1206" value="70uF"/>
<element name="C6" library="evmik_rcl" package="1206" value="70uF"/>
<element name="SWITCH" library="evmik_switches" package="SWITCH1AS" value="SWITCH1AS"/>
<element name="VGAIN" library="evmik_trimmers" package="3362S" value="3362S"/>
<element name="VPHASE" library="evmik_trimmers" package="3362S" value="3362S"/>
<element name="+15V" library="evmik_testpads" package="13" value="TP-13"/>
<element name="-15V" library="evmik_testpads" package="13" value="TP-13"/>
<element name="C3" library="evmik_rcl" package="1206" value="15p"/>
<element name="INVERTER" library="evmik_testpads" package="13" value="TP-13"/>
<element name="R8" library="evmik_rcl" package="1206" value="1k"/>
<element name="R12" library="evmik_rcl" package="1206" value="1k"/>
<element name="REFV" library="evmik_testpads" package="13" value="TP-13"/>
</elements>
<signals>
<signal name="N$6">
<contactref element="INGN" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="VGAIN" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="R2" pad="2"/>
<contactref element="ALPS" pad="6"/>
<contactref element="PHASE" pad="TP"/>
<contactref element="U$1" pad="RA"/>
<contactref element="U$1" pad="RINA"/>
</signal>
<signal name="-15V">
<contactref element="-15V" pad="TP"/>
<contactref element="15_EXT2" pad="3"/>
<contactref element="INGN" pad="4"/>
<contactref element="U$1" pad="-VS"/>
<contactref element="OUT" pad="4"/>
<contactref element="INVT" pad="4"/>
<contactref element="ALPS" pad="4"/>
<contactref element="INBUF" pad="4"/>
<contactref element="15V_EXT1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="R5" pad="1"/>
<contactref element="U$1" pad="RINB"/>
<contactref element="U$1" pad="RB"/>
<contactref element="GND" pad="TP"/>
<contactref element="C2" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="OUTPUT" pad="SHIELD"/>
<contactref element="INPUT" pad="SHIELD"/>
<contactref element="REFERENCE" pad="SHIELD"/>
<contactref element="R9" pad="2"/>
<contactref element="15_EXT2" pad="2"/>
<contactref element="15V_EXT1" pad="2"/>
<contactref element="SWITCH" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="+15V">
<contactref element="INGN" pad="7"/>
<contactref element="ALPS" pad="7"/>
<contactref element="U$1" pad="+VS"/>
<contactref element="+15V" pad="TP"/>
<contactref element="15_EXT2" pad="1"/>
<contactref element="OUT" pad="7"/>
<contactref element="INVT" pad="7"/>
<contactref element="INBUF" pad="7"/>
<contactref element="15V_EXT1" pad="1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="RF"/>
<contactref element="U$1" pad="CHB-"/>
<contactref element="U$1" pad="CHA-"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="VOUT"/>
<contactref element="LIOUT" pad="TP"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R1" pad="2"/>
<contactref element="OUT" pad="3"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="OUT" pad="6"/>
<contactref element="OUT" pad="2"/>
<contactref element="OUTPUT" pad="CONDUCTOR"/>
<contactref element="VOUT" pad="TP"/>
</signal>
<signal name="N$12">
<contactref element="R4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="INVT" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R6" pad="2"/>
<contactref element="VPHASE" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="C1" pad="2"/>
<contactref element="ALPS" pad="3"/>
<contactref element="VPHASE" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="REFERENCE" pad="CONDUCTOR"/>
<contactref element="VREF" pad="TP"/>
<contactref element="R3" pad="1"/>
<contactref element="SWITCH" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="INBUF" pad="2"/>
<contactref element="INBUF" pad="6"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="INPUT" pad="CONDUCTOR"/>
<contactref element="VIN" pad="TP"/>
<contactref element="INBUF" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="C4" pad="2"/>
<contactref element="INGN" pad="3"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="R11" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="R10" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="PREAMP">
<contactref element="VGAIN" pad="2"/>
<contactref element="INGN" pad="6"/>
<contactref element="PREAMP" pad="TP"/>
<contactref element="C1" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="INVT" pad="3"/>
<contactref element="SWITCH" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="ALPS" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R4" pad="2"/>
<contactref element="INVT" pad="6"/>
<contactref element="C3" pad="2"/>
<contactref element="INVERTER" pad="TP"/>
<contactref element="U$1" pad="SELB"/>
</signal>
<signal name="SELA">
<contactref element="R8" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="REFV" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
