<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<library>
<packages>
<package name="SMA-STRAIGHT">
</package>
<package name="CONN-BNC-AMP-TYPE1VERT">
<description>&lt;b&gt;BNC, PCB, vertical&lt;/b&gt;, Amp, e.g. isolated 5227222-6, nut 1-329631-2, lock washer 1-329632-2.&lt;br&gt;
Non-isolated use conn 5227673-1, nut 1-329631-2, lock washer 1-329632-2, shoulder washer 330620.&lt;br&gt;
http://www.tycoelectronics.com</description>
</package>
<package name="CONN-BNC-AMP-TYPE3HORIZ">
<description>&lt;b&gt;BNC PCB &lt;u&gt;Horizontal&lt;/u&gt; mount connector&lt;/b&gt;, Amp, horizontal, 0.1" grid, types such as 227677-1.&lt;br&gt;
Don't forget the nut 1-329631-2 and maybe the shoulder washer 330620.&lt;br&gt;
Now with new &amp; improved mtg holes compared to ...TYPE2...!&lt;br&gt;
The section of the BNC hanging over the edge of the PCB is in layer 49 (Reference).&lt;br&gt;
http://catalog.tycoelectronics.com/TE/bin/TE.Connect?C=1&amp;PN=227677-1&amp;M=STARTSWITH&amp;LG=1&amp;I=13&amp;button.x=0&amp;button.y=0</description>
</package>
</packages>
<symbols>
<symbol name="SMA">
<pin name="CONDUCTOR"/>
<pin name="SHIELD$1"/>
<pin name="SHIELD$2"/>
<pin name="SHIELD$3"/>
<pin name="SHIELD$4"/>
</symbol>
<symbol name="CONN-BNC">
<pin name="CONDUCTOR"/>
<pin name="SHIELD1"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SMA-TYCO-5-1814832-1">
<description>Straight SMA
TYCO ELECTRONICS - 5-1814832-1</description>
<gates>
<gate name="G$1" symbol="SMA"/>
</gates>
<devices>
<device name="" package="SMA-STRAIGHT">
<connects>
<connect gate="G$1" pin="CONDUCTOR" pad="1"/>
<connect gate="G$1" pin="SHIELD$1" pad="G@1"/>
<connect gate="G$1" pin="SHIELD$2" pad="G@2"/>
<connect gate="G$1" pin="SHIELD$3" pad="G@3"/>
<connect gate="G$1" pin="SHIELD$4" pad="G@4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN-BNC">
<description>&lt;b&gt;BNC PCB, horizontal or vertical&lt;/b&gt;, e.g. vertical: Amp 227677-1, nut 1-329631-2, shoulder washer 330620.&lt;br&gt;
The two shield connections allow the assembly on either side of the board.&lt;br&gt;
Horiz isolated: 5227222-6, http://catalog.tycoelectronics.com/TE/bin/TE.Connect?C=1&amp;M=BYPN&amp;TCPN=5227222-6&amp;RQPN=5227222-6
http://catalog.tycoelectronics.com/TE/bin/TE.Connect?C=1&amp;PN=227677-1&amp;M=STARTSWITH&amp;LG=1&amp;I=13&amp;button.x=0&amp;button.y=0&lt;br&gt;
http://catalog.tycoelectronics.com/TE/bin/TE.Connect?C=1&amp;M=BYPN&amp;PID=4946&amp;PN=227673-1&amp;I=13</description>
<gates>
<gate name="." symbol="CONN-BNC"/>
</gates>
<devices>
<device name="-TYPE1VERT" package="CONN-BNC-AMP-TYPE1VERT">
<connects>
<connect gate="." pin="CONDUCTOR" pad="CONDUCTOR"/>
<connect gate="." pin="SHIELD1" pad="SHIELD1 SHIELD2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESC" value="Input?"/>
</technology>
</technologies>
</device>
<device name="TYPE3HORIZ" package="CONN-BNC-AMP-TYPE3HORIZ">
<connects>
<connect gate="." pin="CONDUCTOR" pad="CONDUCTOR"/>
<connect gate="." pin="SHIELD1" pad="SHIELD1 SHIELD2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
