From 5e32fa95cec1734ebe84ca60d627e49c705cb555 Mon Sep 17 00:00:00 2001
From: Eugeniy Mikhailov <evgmik@gmail.com>
Date: Thu, 4 Sep 2014 19:28:36 -0400
Subject: typo fix, thanks Caroline

---
 interferometry.tex | 4 +++-
 1 file changed, 3 insertions(+), 1 deletion(-)

(limited to 'interferometry.tex')

diff --git a/interferometry.tex b/interferometry.tex
index 507a396..ef14794 100644
--- a/interferometry.tex
+++ b/interferometry.tex
@@ -175,7 +175,9 @@ you will use it to measure the wavelength of strong yellow sodium
 fluorescent light, produced by the discharge lamp.\footnote{Actually,
 sodium might be a better calibration source than a HeNe laser, since it has well known lines, whereas a HeNe can lase at different wavelengths.  Perhaps an even better calibration source might be a line from the Hydrogen Balmer series, which can be calculated from the Standard Model.}
 
-Without changing the alignment of the interferometer (i.e. without touching any mirrors), remove the focusing lens and carefully place the interferometer assembly on top of an adjustable-hight platform such that it is at the same level as the output of the lamp. Since the light power in this case is much weaker than for a laser, you won't be able to use the viewing screen. You will have to observe the interference looking directly to the output beam - unlike laser radiation, the spontaneous emission of a discharge is not dangerous\footnote{In the ``old days'' beams in high energy physics were aligned using a similar technique. An experimenter would close his eyes and then put his head in a collimated particle beam. Cerenkov radiation caused by particles traversing the experimenter's eyeball is visible as a blue glow or flashes. This is dangerous but various people claim to have done it... when a radiation safety officer isn't around.}  However, your eyes will get tired quickly! Placing a diffuser plate in front of the lamp will make the observations easier. Since the interferometer is already aligned, you should see the interference picture. Make small adjustments to the adjustable mirror to make sure you see the center of the bull's eye.
+Without changing the alignment of the interferometer (i.e. without touching
+any mirrors), remove the focusing lens and carefully place the
+interferometer assembly on top of an adjustable-height platform such that it is at the same level as the output of the lamp. Since the light power in this case is much weaker than for a laser, you won't be able to use the viewing screen. You will have to observe the interference looking directly to the output beam - unlike laser radiation, the spontaneous emission of a discharge is not dangerous\footnote{In the ``old days'' beams in high energy physics were aligned using a similar technique. An experimenter would close his eyes and then put his head in a collimated particle beam. Cerenkov radiation caused by particles traversing the experimenter's eyeball is visible as a blue glow or flashes. This is dangerous but various people claim to have done it... when a radiation safety officer isn't around.}  However, your eyes will get tired quickly! Placing a diffuser plate in front of the lamp will make the observations easier. Since the interferometer is already aligned, you should see the interference picture. Make small adjustments to the adjustable mirror to make sure you see the center of the bull's eye.
 
 Repeat the same measurements as in the previous part by moving the mirror and counting the number of fringes. Each lab partner should make at least two independent measurements, recording initial and final position of the micrometer, and you should do at least five trials. Calculate the wavelength of the Na light for each trial. Then calculate the average value and its experimental uncertainty. Compare with the expected value of \unit[589]{nm}.
 
-- 
cgit v1.2.3

