From c12868d67f4e9dc450564eaf57c0352b9cc2989a Mon Sep 17 00:00:00 2001
From: "Eugeniy E. Mikhailov" <evgmik@gmail.com>
Date: Wed, 11 Sep 2019 22:57:42 -0400
Subject: change figure size to fit in a page

---
 interferometry.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'interferometry.tex')

diff --git a/interferometry.tex b/interferometry.tex
index 7ca903f..c55c206 100644
--- a/interferometry.tex
+++ b/interferometry.tex
@@ -210,7 +210,7 @@ In reality, the Na discharge lamp produces a doublet - two spectral lines that a
 
 \begin{figure}
 \centering
-\includegraphics[width=0.8\linewidth]{./pdf_figs/fpfig3} \caption{\label{fpfig3.fig}The Fabry-Perot Interferometer.  \textbf{For initial alignment the laser and the convex lens are used instead of the Na lamp.}}
+\includegraphics[width=0.7\linewidth]{./pdf_figs/fpfig3} \caption{\label{fpfig3.fig}The Fabry-Perot Interferometer.  \textbf{For initial alignment the laser and the convex lens are used instead of the Na lamp.}}
 \end{figure}
 Disassemble the Michelson Interferometer, and assemble the Fabry-Perot interferometer as shown in
 Figure~\ref{fpfig3.fig}, initially using the laser for alignment instead of the sodium lamp. First, place the viewing screen behind the two partially-reflecting mirrors ($P1$ and $P2$), and adjust the mirrors such
@@ -284,7 +284,7 @@ Use this equation and your experimental measurements to calculate average value
 
 \begin{figure}[h]
 \centering
-\includegraphics[width=0.7\linewidth]{./pdf_figs/fpfig4} 
+\includegraphics[width=0.60\linewidth]{./pdf_figs/fpfig4} 
 \\
 	\centering
 	\begin{subfigure}[t]{0.18\textwidth}
-- 
cgit v1.2.3

