From 96435b51234dac8ef8817db7487cc77a7003aed8 Mon Sep 17 00:00:00 2001
From: Eugeniy Mikhailov <evgmik@gmail.com>
Date: Fri, 30 Aug 2013 17:29:34 -0400
Subject: fixed wrong scale for micrometer in the text

---
 manual/chapters/interferometry.tex | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

(limited to 'manual/chapters/interferometry.tex')

diff --git a/manual/chapters/interferometry.tex b/manual/chapters/interferometry.tex
index bc85141..112e493 100644
--- a/manual/chapters/interferometry.tex
+++ b/manual/chapters/interferometry.tex
@@ -132,7 +132,8 @@ Once the interferometer is aligned, insert a convex lens ($f=\unit[18]{mm}$ work
 \textbf{Note}: before starting the measurements, make sure you understand how to read the micrometer properly!
 \begin{figure}[h]
 \centering
-\includegraphics[width=0.7\columnwidth]{./pdf_figs/fig3} \caption{\label{fig3mich.fig}Micrometer readings. The course scale is in mm, and smallest division on the rotary dial is 1~$\mu$m (same as 1 micron). The final measurements is the sum of two. }
+\includegraphics[width=0.7\columnwidth]{./pdf_figs/fig3}
+\caption{\label{fig3mich.fig}Micrometer readings. The course division equals to 100~$\mu$m, and smallest division on the rotary dial is 1~$\mu$m (same as 1 micron). The final measurements is the sum of two. }
 \end{figure}
 
 \section*{Wavelength measurements using Michelson interferometer}
-- 
cgit v1.2.3

