From 588e91859f468ea6fbfdc846a9146dcffcfecedc Mon Sep 17 00:00:00 2001
From: Eugeniy Mikhailov <evgmik@gmail.com>
Date: Tue, 3 Sep 2013 18:17:11 -0400
Subject: typos fixed in emratio chapter

---
 manual_source/chapters/emratio.tex | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

(limited to 'manual_source/chapters/emratio.tex')

diff --git a/manual_source/chapters/emratio.tex b/manual_source/chapters/emratio.tex
index e262b7e..fc3c716 100644
--- a/manual_source/chapters/emratio.tex
+++ b/manual_source/chapters/emratio.tex
@@ -44,8 +44,8 @@
 
 
 \section*{Theory}
-         The apparatus shown in Figure \ref{emfig1}.
-consists of a glass tube that
+         The apparatus shown in Figure \ref{emfig1}
+	 consists of a glass tube that
         houses a small electron gun.  This gun has a cathode filament
         from which electrons can be thermionically released (boiled
         off), and a nearby anode which can be set to a potential which
@@ -142,7 +142,7 @@ electron beam.
 The Helmholtz coils of the $e/m$ apparatus have a radius and separation of
 $a=15$~cm. Each coil has $N=130$~turns. The magnetic field ($B$) produced by
 the coils is proportional to the current through the coils ($I_{hc}$) times
-$7.80\cdot10^{-4}$~tesla/ampere [$B (tesla) = (7.80 \cdot 10^{-4}) I_{hc}$]. A
+$7.80\cdot10^{-4}$~Tesla/Ampere [$B (tesla) = (7.80 \cdot 10^{-4}) I_{hc}$]. A
 mirrored scale is attached to the back of the rear Helmholtz coil. It is
 illuminated automatically when the heater of the electron
 gun is powered. By lining the electron beam up with its image in the mirrored
-- 
cgit v1.2.3

