<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<library>
<packages>
<package name="SOIC8">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
<package name="DIP8">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="OPAMP_GENERIC">
<pin name="OPT3" direction="pas"/>
<pin name="OPT2" direction="pas"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="OPT1" direction="pas"/>
<pin name="V+" direction="in"/>
<pin name="V-" direction="in"/>
</symbol>
<symbol name="INA128">
<pin name="REF" direction="pas"/>
<pin name="RG2" direction="pas"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="RG1" direction="pas"/>
<pin name="V+" direction="in"/>
<pin name="V-" direction="in"/>
</symbol>
<symbol name="OPAMP_SIMPLE">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="OPAMP_ADA4817">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="PD" direction="pas"/>
<pin name="FB" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="OPAMP_GENERIC" prefix="IC" uservalue="yes">
<description>Generic 8 pin opamp like u741, opa27 or opa37</description>
<gates>
<gate name="G$1" symbol="OPAMP_GENERIC"/>
</gates>
<devices>
<device name="SOIC8" package="SOIC8">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OPT1" pad="1"/>
<connect gate="G$1" pin="OPT2" pad="8"/>
<connect gate="G$1" pin="OPT3" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DIP8" package="DIP8">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OPT1" pad="1"/>
<connect gate="G$1" pin="OPT2" pad="8"/>
<connect gate="G$1" pin="OPT3" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA128" prefix="INA128">
<gates>
<gate name="G$1" symbol="INA128"/>
</gates>
<devices>
<device name="DIP8" package="DIP8">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG1" pad="1"/>
<connect gate="G$1" pin="RG2" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOIC8" package="SOIC8">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG1" pad="1"/>
<connect gate="G$1" pin="RG2" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPAMP_GENERIC_SIMPLE" uservalue="yes">
<gates>
<gate name="G$1" symbol="OPAMP_SIMPLE"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADA4817">
<gates>
<gate name="G$1" symbol="OPAMP_ADA4817"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="FB" pad="1"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="PD" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
